Not found in iOS file
 
CHARACTERISTIC_PROPERTIES_SIGNED_WRITES
Permits signed writes of the characteristic value.
platforms: [iphone, ipad, android]

CONNECTION_TIMEOUT_ERROR Number
 One of the possible values of the errorCode property of an event in case an error occurs.

ERROR_DOMAIN
One of the possible values of the errorDomain property of an event in case an error occurs.

INVALID_HANDLE_ERROR Number
 One of the possible values of the errorCode property of an event in case an error occurs.

INVALID_PARAMETERS_ERROR Number
One of the possible values of the errorCode property of an event in case an error occurs.

ALREADY_ADVERTISING_ERROR
One of the possible values of the errorCode property of an event in case an error occurs.

ATT_ERROR_DOMAIN
One of the possible values of the errorDomain property of an event in case an error occurs.

BACKGROUND_DATA_AUTHORIZATION_STATUS_AUTHORIZED Number  One of the possible values of the backgroundDataAuthorizationStatus property. User has authorized this application to share data while backgrounded. 
BACKGROUND_DATA_AUTHORIZATION_STATUS_DENIED Number  One of the possible values of the backgroundDataAuthorizationStatus property. User has explicitly denied this application from sharing data while backgrounded. 
BACKGROUND_DATA_AUTHORIZATION_STATUS_NOT_DETERMINED Number  One of the possible values of the backgroundDataAuthorizationStatus property. User has not yet made a choice with regards to this application. 
BACKGROUND_DATA_AUTHORIZATION_STATUS_RESTRICTED Number  One of the possible values of the backgroundDataAuthorizationStatus property. This application is not authorized to share data while backgrounded. The user cannot change this application’s status, possibly due to active restrictions such as parental controls being in place. 
BEACON_PROXIMITY_FAR Number One of the possible values of the proximity property. platforms: [iphone, ipad, android] 
BEACON_PROXIMITY_IMMEDIATE Number One of the possible values of the proximity property. platforms: [iphone, ipad, android] 
BEACON_PROXIMITY_NEAR Number  One of the possible values of the proximity property. platforms: [iphone, ipad, android] 
BEACON_PROXIMITY_UNKNOWN Number  One of the possible values of the proximity property. platforms: [iphone, ipad, android] 
CENTRAL_MANAGER_SCAN_OPTION_KEY_ALLOW_DUPLICATES String
 Use this constant as a key in the options parameter of the startScan. The value associated with this key is a number, indicating whether the scan should run without duplicate filtering. By default, multiple discoveries of the same peripheral are coalesced into a single discovery event. Disabling this filtering can have an adverse effect on battery life and should only be used if necessary.

MANAGER_STATE_UNINITIALIZED Number
This state is reported when the central manager object maintained by the module does not (yet) exist, i.e. before initCentralManageris called or after releaseCentralManageris called. platforms: [iphone, ipad]

CHARACTERISTIC_PERMISSION_NONE Number
Characteristic has no permissions.
platforms: [iphone, ipad, android]

LOCATION_MANAGER_AUTHORIZATION_STATUS_AUTHORIZED Number One of the possible values of the locationManagerAuthorizationStatus property. User has authorized this application to share data while backgrounded. 
LOCATION_MANAGER_AUTHORIZATION_STATUS_DENIED Number One of the possible values of the locationManagerAuthorizationStatus property. The user explicitly denied the use of location services for this application or location services are currently disabled in Settings. 
LOCATION_MANAGER_AUTHORIZATION_STATUS_NOT_DETERMINED Number One of the possible values of the locationManagerAuthorizationStatus property. The user has not yet made a choice regarding whether this application can use location services. 
LOCATION_MANAGER_AUTHORIZATION_STATUS_RESTRICTED Number  One of the possible values of the locationManagerAuthorizationStatus property. The user cannot change this application’s status, possibly due to active restrictions such as parental controls being in place. 
NOT_CONNECTED_ERROR Number  One of the possible values of the errorCode property of an event in case an error occurs. 
OPERATION_CANCELLED_ERROR Number One of the possible values of the errorCode property of an event in case an error occurs. 
OUT_OF_SPACE_ERROR Number One of the possible values of the errorCode property of an event in case an error occurs.

PERIPHERAL_DISCONNECTED_ERROR Number
 One of the possible values of the errorCode property of an event in case an error occurs.

PERIPHERAL_STATE_CONNECTED Number
One of the possible values of the state property of a peripheral object.

PERIPHERAL_STATE_CONNECTING Number  One of the possible values of the state property of a peripheral object. 
PERIPHERAL_STATE_DISCONNECTED Number One of the possible values of the state property of a peripheral object. 

REGION_STATE_INSIDE Number One of the possible values of the state property of the regionStateUpdated event. platforms: [iphone, ipad, android] 
REGION_STATE_OUTSIDE Number One of the possible values of the state property of the regionStateUpdated event. platforms: [iphone, ipad, android] 
REGION_STATE_UNKNOWN Number One of the possible values of the state property of the regionStateUpdated event. platforms: [iphone, ipad, android] 
UNKNOWN_ERROR Number One of the possible values of the errorCode property of an event in case an error occurs. 
UUID_NOT_ALLOWED_ERROR Number One of the possible values of the errorCode property of an event in case an error occurs. 
CONNECTION_PRIORITY_BALANCED Number Use this constant for the type parameter of the requestConnectionPriority method. It specifies the priority for the request of the remote device platforms: [android] 
CONNECTION_PRIORITY_HIGH Number Use this constant for the type parameter of the requestConnectionPriority method. It specifies the priority for the request of the remote device platforms: [android] 
CONNECTION_PRIORITY_LOW_POWER Number Use this constant for the type parameter of the requestConnectionPriority method. It specifies the priority for the request of the remote device platforms: [android] 
DISABLE_NOTIFICATION_VALUE TiBuffer Value used to disable notifications or indications for a client configuration descriptor. You may pass this constant to the unsubscribeFromCharacteristic method. platforms: [android] 
ENABLE_INDICATION_VALUE TiBuffer Value used to enable indication for a client configuration descriptor. You may pass this constant to the subscribeToCharacteristic method. platforms: [android] 
ENABLE_NOTIFICATION_VALUE TiBuffer Value used to enable notification for a client configuration descriptor. You may pass this constant to the subscribeToCharacteristic method. platforms: [android]